**Standard Freight Trailer**

## Standards:

**Common Lengths:** 28-53 feet

**Width:** 96 - 102 inches

**Height:** 12.5 - 13.5 feet

**Door Type:** Swing Door/Roller door (equip varies by carrier)

## Capacity:

**Max Weight @ 53 ft length:**

45,000 lbs

**Max Pallets @ 53 ft:** 26 pallets

## Usage:

Used to carry most common

freight (boxed, crated, palletized, etc.)

# Common Standard Freight Trailer Specifications

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | **Overall** |  |  | **Interior** |  | **Rear Door** | **Capacity** | **Max Weight** |
| Length | Width | Height | Length | Width | Height | Width | Height |  |  |
| 40 ft | 96” | 12’ 6” | 39’ 6” | 92.5” | 94.5” | 92” | 92” | 2,398 cu ft | 11,300 lbs |
| 43 ft | 96” | 13’ 0” | 41’ 6” | 92.5” | 100.5” | 92” | 98” | 2,711 cu ft | 11,900 lbs |
| 48 ft | 102” | 13’ 6” | 47’ 6” | 98.5” | 100.6” | 98” | 100.6” | 3,465 cu ft | 13,500 lbs |
| 53 ft | 102” | 13’ 6” | 47’ 6” | 98.5” | 108” | 94” | 102” | 3,489 cu ft | 13,500 lbs |

Data provided for illustrative purposes only. Actual equipment in use varies by carrier and manufacturer. This is only a guide and should not be used as a definitive reference for dock planning.

**Straight Truck**

## Standards:

**Common Lengths:** 22-26 feet

**Width:** 96 - 102 inches

**Height:** 12.5 - 13.5 feet

**Door Type:** Swing Door/Roller Door (varies by carrier)

## Capacity:

**Max Weight @ 26 ft length:**

14,000 lbs

**Max Pallets @ 26 ft:** 12 pallets

## Usage:

**Available Options:**

Lift Gate

Refrigeration

**Pup Trailer**

## Standards:

**Common Lengths:** 28 feet

**Width:** 96 - 102 inches

**Height:** 12.5 - 13.5 feet

**Door Type:** Swing Door/Roller Door (varies by carrier)

## Capacity:

**Max Weight @ 28 ft length:**

22,000 lbs

**Max Pallets @ 28 ft:** 14 pallets

## Usage:

**Available Options:**

Lift Gate

Single, Tandem & Triple

**Shipping Container**


## Standards:

20 ft

**Common Lengths:** 20, 40, 45, 48, 53 feet

40 ft

**Width:** 98 - 102 inches

**Height:** 8.5 — 9.5 feet

**Door Type:** Swing Door

45 ft

## Capacity:

**Max Weight @ 40 ft length:** 71,390 lbs

48 ft

## Usage:

Designed to transport cargo internationally

53 ft

# Common Shipping Container Specifications

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  | **20’** | **40’** | **45’** | **48’** | **53’** |
| **Length** | 19’ 10” | 40’ | 45’ | 48’ | 53’ |
| **Inside Length** | 19’ 4” | 39’ 6” | 44.6’ | 47.6’ | 52.3’’ |
| **Height** | 8’ 6” | 8’ 6” | 9’ 6” | 9’ 6” | 9’ 6” |
| **Inside Height** | 7’ 9” | 7’ 10” | 8’ 10” | 8’ 10” | 8’ 10” |
| **Door (H x W)** | 7’6” X 7’ 8” | 7’6” X 7’ 8” | 8’ 6” X 7’ 8” | 8’ 6” X 7’ 8” | 8’ 6” X 7’ 8” |
| **Width** | 8’ | 8’ | 8’ | 8’ 6” | 8’ 6” |
| **Inside Width** | 7’ 8” | 7’ 8’ | 7’ 8” | 8’ 2” | 8’ 2” |
| **Capacity** | 1,170 ft3 | 2,390 ft3 | 2,700 ft3 | 3,000 ft3 | 3,800 ft3 |

Data provided for illustrative purposes only. Actual equipment in use varies by carrier and manufacturer. This is only a guide and should not be used as a definitive reference for dock planning.